*QUESTIONS AND ANSWERS FOR ELECTRICAL MAINTENANCE AND REPAIR BID (GPAA 04 2020)*

|  |  |  |
| --- | --- | --- |
| NO | QUESTION | ANSWER |
| 1 | UPS power plugs (specific size) | 32A 3pin caravan plug |
| 2 | Air conditioner isolator (specs) | 2x4 x 20A isolator |
| 3 | Type of a magnetic door lock- magnetic lock | 300kg holding lock |
| 4 | Motion sensor(specs) | PIR 36 ceiling infrared motion sensor 360degrees (1100w) |
| 5 | Down lighters (type | MR16 LED down light fitting (silver chrome) |
| 6 | Fluorescent lights (type) | 4ft 2x35w surface mounted LED fluorescent light |
| 7 | Pole lights(type) | 250w LED pole light |
| 8 | flood lights "they require flood light to match the existing one " at least if we could get a pictures | 400W LED restin 4 outdoor flood light |
| 9 | UPS replacement batteries (size /specs) | 12v 200Ah, 2,25v pc @ 25 degrees Celsius, 8N.m |
| 10 | Generator replacement batteries (size/specs) | 12v 102 Ah, RC 180min, CCA (-18 degree Celsius) EN/SAE :710A, 15Nm. |